{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["报价函"],"read":"whole","date_system":"1900"}

{"sheet":"报价函","index":0,"n_rows":121,"n_cols":10,"rows_kept":121,"merged":[[0,0,0,6]]}
["报价表"]
["序号","项目名称","单位","工程量","单价（元）","合价（元）","备注"]
[1,"DN250PE给水管","m",1960,null,null,"PE（PE100）0.8MPa"]
[2,"DN200PE给水管","m",135,null,null,"PE（PE100）0.8MPa"]
[3,"DN160PE给水管","m",738,null,null,"PE（PE100）0.8MPa"]
[4,"DN110PE给水管","m",9320,null,null,"PE（PE100）0.8MPa"]
[5,"DN90PE给水管","m",16544,null,null,"PE（PE100）1.0MPa"]
[6,"DN75PE给水管","m",15303,null,null,"PE（PE100）1.25MPa"]
[7,"DN50PE给水管","m",37384,null,null,"PE（PE100）1.60MPa"]
[8,"DN32PE给水管","m",7750,null,null,"PE（PE100）1.60MPa"]
[9,"DN20PE给水管","m",8000,null,null,"PE（PE100）1.60MPa"]
[10,"DN20PPR供水管","m",1]
[11,"PE20外丝直接","个",1]
[12,"PPR20外丝直接","个",1]
[13,"PPR20内丝直接","个",1]
[14,"DN20PPR弯头（90°）","个",1]
[15,"DN20PPR直接","个",1]
[16,"PPR20内丝弯头","个",1]
[17,"入户闸阀（DN20PE截止阀）","个",1]
[18,"入户锁阀（磁性锁闭铜球阀）","个",1]
[19,"DN15水龙头","个",1]
[20,"保温棉","m",1]
[21,"勾钉","个",1]
[22,"DN250闸阀","个",2,null,null,"铁质铜芯PN=1.0MPa，法兰连接，含配套法兰"]
[23,"DN200闸阀","个",1,null,null,"铁质铜芯PN=1.0MPa，法兰连接，含配套法兰"]
[24,"DN160闸阀","个",1,null,null,"铁质铜芯PN=1.0MPa，法兰连接，含配套法兰"]
[25,"DN110闸阀","个",22,null,null,"铁质铜芯PN=1.0MPa，法兰连接，含配套法兰"]
[26,"DN90闸阀","个",33,null,null,"铁质铜芯PN=1.0MPa，法兰连接，含配套法兰"]
[27,"DN75闸阀","个",31,null,null,"铁质铜芯PN=1.0MPa，法兰连接，含配套法兰"]
[28,"DN50闸阀","个",12,null,null,"铁质铜芯PN=1.0MPa，螺纹连接，含配套法兰"]
[29,"DN110排污阀","个",1,null,null,"铁质铜芯PN=1.0MPa，法兰连接，含配套法兰"]
[30,"DN75排污阀","个",40,null,null,"铁质铜芯PN=1.0MPa，法兰连接，含配套法兰"]
[31,"DN50排污阀","个",6,null,null,"铁质铜芯PN=1.0MPa，法兰连接，含配套法兰"]
[32,"φ1200mm阀门井","个",101,null,null,"防坠安全网、\n球墨铸铁井盖等"]
[33,"600*600mm排污阀井","个",47,null,null,"防坠安全网、\n球墨铸铁井盖等"]
[34,"SS100室外消火栓","个",21]
[35,"φ15Emm数字水表 入\n户改造","组",692,null,null,"室外水表井（高分子材\n料）400*600*400\n宽*长*深",null,null,"    "]
[36,"φ15Emm数字水表 入\n户改造","组",692,null,null,"水表及配件采购"]
[37,"φ15Emm数字水表 入\n户改造","组",160,null,null,"室外水表井（高分子材\n料）400*600*400\n宽*长*深"]
[38,"φ15Emm数字水表 入\n户改造","组",160,null,null,"水表及配件采购"]
[39,"φ15Emm智能冷水水表 入户改造","组",33,null,null,"室外水表井（高分子材\n料）400*600*400\n宽*长*深"]
[40,"φ15Emm智能冷水水表 入户改造","组",33,null,null,"水表及配件采购"]
[41,"φ20Emm智能冷水水表 入户改造","组",200,null,null,"水表及配件采购"]
[42,"φ25Emm智能冷水水表 入户改造","组",96,null,null,"水表及配件采购"]
[43,"φ32Emm智能冷水水表 入户改造","组",66,null,null,"水表及配件采购"]
[44,"φ40Emm智能冷水水表 入户改造","组",15,null,null,"水表及配件采购"]
[45,"φ50Emm智能冷水水表 入户改造","组",60,null,null,"水表及配件采购"]
[46,"T250-250-T250","个",1]
[47,"T200-200-T200","个",1]
[48,"T160-160-T160","个",1]
[49,"T110-110-T110","个",1]
[50,"T90-90-T90","个",1]
[51,"T75-75-T75","个",1]
[52,"T50-50-T50","个",1]
[53,"T32-32-T32","个",1]
[54,"T20-20-T20","个",1]
[55,"S32-20","个",1]
[56,"S50-20","个",1]
[57,"S50-32","个",1]
[58,"S75-32","个",1]
[59,"S75-50","个",1]
[60,"S90-50","个",1]
[61,"S90-75","个",1]
[62,"S110-50","个",1]
[63,"S110-75","个",1]
[64,"S110-90","个",1]
[65,"S160-110","个",1]
[66,"S160-50","个",1]
[67,"S160-75","个",1]
[68,"S160-90","个",1]
[69,"S200-160","个",1]
[70,"S200-110","个",1]
[71,"S200-90","个",1]
[72,"S200-75","个",1]
[73,"S200-50","个",1]
[74,"S250-200","个",1]
[75,"S250-160","个",1]
[76,"S250-110","个",1]
[77,"S250-90","个",1]
[78,"S250-75","个",1]
[79,"S250-50","个",1]
[80,"T250-200-T250","个",1]
[81,"T250-160-T250","个",1]
[82,"T250-110-T250","个",1]
[83,"T250-90-T250","个",1]
[84,"T250-75-T250","个",1]
[85,"T250-50-T250","个",1]
[86,"T200-160-T200","个",1]
[87,"T200-110-T200","个",1]
[88,"T200-90-T200","个",1]
[89,"T200-75-T200","个",1]
[90,"T200-50-T200","个",1]
[91,"T160-90-T160","个",1]
[92,"T160-75-T160","个",1]
[93,"T160-110-T160","个",1]
[94,"T160-50-T160","个",1]
[95,"T110-90-T110","个",1]
[96,"T110-75-T110","个",1]
[97,"T110-50-T110","个",1]
[98,"T110-32-T110","个",1]
[99,"T90-75-T90","个",1]
[100,"T90-50-T90","个",1]
[101,"T90-32-T90","个",1]
[102,"T75-50-T75","个",1]
[103,"T75-32-T75","个",1]
[104,"T50-32-T50","个",1]
[105,"T50-20-T50","个",1]
[106,"T32-20-T32","个",1]
[107,"L250×90°  ","个",1]
[108,"L200×90°  ","个",1]
[109,"L160×90°  ","个",1]
[110,"L110×90°  ","个",1]
[111,"L90×90°  ","个",1]
[112,"L75×90°  ","个",1]
[113,"L50×90°  ","个",1]
[114,"L32×90°  ","个",1]
[115,"L20×90°  ","个",1]
[116,"直接PE20","只",1]
[117,"直接PE32","只",1]
[118,"直接PE50","只",1]
[119,"直接PE75","只",1]